Ballpoint Pen

1. Test the ink chamber is fulfilled
2. Test the joint of socket with the ink chamber
3. Test the ball on socket is working properly
4. Test the ink is coming out properly
5. Test the functionality of spring
6. Test the adjustment of thrust devices (thrust device + thrust tube)
7. Test the adjustment of pen tip with the pen grip
8. Test the pen barrel contain thrust devices properly
9. Test the plunge is working perfectly (after joining all the devices)
10. Test the pen grip is comfortable for writing
11. Test the pen clip is easy to hang
12. Test the functionality of the pen after is dropped down from hand (!)